HOST-RESOURCES-TYPES DEFINITIONS ::= BEGIN

IMPORTS
  MODULE-IDENTITY, OBJECT-IDENTITY        FROM SNMPv2-SMI
  hrMIBAdminInfo, hrStorage, hrDevice     FROM HOST-RESOURCES-MIB;

hostResourcesTypesModule MODULE-IDENTITY
  LAST-UPDATED "200003060000Z"    -- 6 March, 2000
  ORGANIZATION "IETF Host Resources MIB Working Group"
  CONTACT-INFO
      "Steve Waldbusser
      Postal: Lucent Technologies, Inc.
              1213 Innsbruck Dr.
              Sunnyvale, CA 94089
              USA
      Phone: 650-318-1251
      Fax:   650-318-1633
      Email: waldbusser@ins.com

      In addition, the Host Resources MIB mailing list is dedicated
      to discussion of this MIB. To join the mailing list, send a
      request message to hostmib-request@andrew.cmu.edu. The mailing
      list address is hostmib@andrew.cmu.edu."
  DESCRIPTION
      "This MIB module registers type definitions for
      storage types, device types, and file system types.

      After the initial revision, this module will be
      maintained by IANA."
  REVISION "200003060000Z"    -- 6 March 2000
  DESCRIPTION
      "The original version of this module, published as RFC
      2790."
  ::= { hrMIBAdminInfo 4 }

-- Registrations for some storage types, for use with hrStorageType
hrStorageTypes          OBJECT IDENTIFIER ::= { hrStorage 1 }

hrStorageOther OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used when no other defined
        type is appropriate."
    ::= { hrStorageTypes 1 }

hrStorageRam OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for RAM."
    ::= { hrStorageTypes 2 }

hrStorageVirtualMemory OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for virtual memory,
        temporary storage of swapped or paged memory."
    ::= { hrStorageTypes 3 }

hrStorageFixedDisk OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for non-removable
        rigid rotating magnetic storage devices."
    ::= { hrStorageTypes 4 }

hrStorageRemovableDisk OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for removable rigid
        rotating magnetic storage devices."
    ::= { hrStorageTypes 5 }

hrStorageFloppyDisk OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for non-rigid rotating
        magnetic storage devices."
    ::= { hrStorageTypes 6 }

hrStorageCompactDisc OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for read-only rotating
        optical storage devices."
    ::= { hrStorageTypes 7 }

hrStorageRamDisk OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for a file system that
        is stored in RAM."
    ::= { hrStorageTypes 8 }

hrStorageFlashMemory OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for flash memory."
    ::= { hrStorageTypes 9 }

hrStorageNetworkDisk OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The storage type identifier used for a
        networked file system."
    ::= { hrStorageTypes 10 }

-- Registrations for some device types, for use with hrDeviceType
hrDeviceTypes             OBJECT IDENTIFIER ::= { hrDevice 1 }

hrDeviceOther OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used when no other defined
        type is appropriate."
    ::= { hrDeviceTypes 1 }

hrDeviceUnknown OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used when the device type is
        unknown."
    ::= { hrDeviceTypes 2 }

hrDeviceProcessor OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a CPU."
    ::= { hrDeviceTypes 3 }

hrDeviceNetwork OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a network interface."
    ::= { hrDeviceTypes 4 }

hrDevicePrinter OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a printer."
    ::= { hrDeviceTypes 5 }

hrDeviceDiskStorage OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a disk drive."
    ::= { hrDeviceTypes 6 }

hrDeviceVideo OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a video device."
    ::= { hrDeviceTypes 10 }

hrDeviceAudio OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for an audio device."
    ::= { hrDeviceTypes 11 }

hrDeviceCoprocessor OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a co-processor."
    ::= { hrDeviceTypes 12 }

hrDeviceKeyboard OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a keyboard device."
    ::= { hrDeviceTypes 13 }

hrDeviceModem OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a modem."
    ::= { hrDeviceTypes 14 }

hrDeviceParallelPort OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a parallel port."
    ::= { hrDeviceTypes 15 }

hrDevicePointing OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a pointing device
        (e.g., a mouse)."
    ::= { hrDeviceTypes 16 }

hrDeviceSerialPort OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a serial port."
    ::= { hrDeviceTypes 17 }

hrDeviceTape OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a tape storage device."
    ::= { hrDeviceTypes 18 }

hrDeviceClock OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a clock device."
    ::= { hrDeviceTypes 19 }

hrDeviceVolatileMemory OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a volatile memory
        storage device."
    ::= { hrDeviceTypes 20 }

hrDeviceNonVolatileMemory OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
        "The device type identifier used for a non-volatile memory

        storage device."
    ::= { hrDeviceTypes 21 }

-- Registrations for some popular File System types,
-- for use with hrFSType.
hrFSTypes               OBJECT IDENTIFIER ::= { hrDevice 9 }

hrFSOther OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used when no other
        defined type is appropriate."
    ::= { hrFSTypes 1 }

hrFSUnknown OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used when the type of
        file system is unknown."
    ::= { hrFSTypes 2 }

hrFSBerkeleyFFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Berkeley Fast File System."
    ::= { hrFSTypes 3 }

hrFSSys5FS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        System V File System."
    ::= { hrFSTypes 4 }

hrFSFat OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for
        DOS's FAT file system."
    ::= { hrFSTypes 5 }

hrFSHPFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for OS/2's
        High Performance File System."
    ::= { hrFSTypes 6 }

hrFSHFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Macintosh Hierarchical File System."
    ::= { hrFSTypes 7 }

hrFSMFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Macintosh File System."
    ::= { hrFSTypes 8 }

hrFSNTFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Windows NT File System."
    ::= { hrFSTypes 9 }

hrFSVNode OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        VNode File System."
    ::= { hrFSTypes 10 }

hrFSJournaled OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Journaled File System."
    ::= { hrFSTypes 11 }

hrFSiso9660 OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        ISO 9660 File System for CD's."
    ::= { hrFSTypes 12 }

hrFSRockRidge OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        RockRidge File System for CD's."
    ::= { hrFSTypes 13 }

hrFSNFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        NFS File System."
    ::= { hrFSTypes 14 }

hrFSNetware OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Netware File System."
    ::= { hrFSTypes 15 }

hrFSAFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Andrew File System."
    ::= { hrFSTypes 16 }

hrFSDFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        OSF DCE Distributed File System."
    ::= { hrFSTypes 17 }

hrFSAppleshare OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        AppleShare File System."
    ::= { hrFSTypes 18 }

hrFSRFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        RFS File System."
    ::= { hrFSTypes 19 }

hrFSDGCFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Data General DGCFS."
    ::= { hrFSTypes 20 }

hrFSBFS OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        SVR4 Boot File System."
    ::= { hrFSTypes 21 }

hrFSFAT32 OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Windows FAT32 File System."
    ::= { hrFSTypes 22 }

hrFSLinuxExt2 OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The file system type identifier used for the
        Linux EXT2 File System."
    ::= { hrFSTypes 23 }

END
